- Download the init script for CallCabinet and place it in

/etc/init.d/ccinitd on the PBXWare server

- Ensure that the script is executable:

- chmod +x /etc/init.d/ccinitd

- Add the script to the system boot sequence:

- rc-update add ccinitd default

- **OR** try below script to the system boot sequence::

- update-rc.d ccinitd default